Tritec Electronic AG, Germany

Readme version 3.2 Date 12.11.2018 JB


Installation instruction for 'ADIO Service Tool' Version 3.2 for Windows 

For details how to use the 'ADIO Service Tool' refer to the ADIO manual.

Package content:
File: Readme.txt			this readme document
File: CDM21218_Setup			Setup up for drivers of the USB serial communication
File: ADIO_service_tool.exe		ADIO Service Tool Version 3.2, Executable file

Installation:
	- Start the 'CDM21218_Setup' file and follow the instructions.
	- Connect the ADIO Tx-board with a USB to mini USB cable to the PC and power it up.
	- Wait a few seconds that Windows can load the drivers.
	- Start the 'ADIO_service_tool'
	- Do not unzip the ADIO_FW_Version file. 
	
If there is more than one USB-serial connection available select the appropriate com port 
under 'available devices' in the lower left corner.



 